# Sentinel® LDK and Sentinel HASP® Run-time Environment Installer GUI for Windows: Readme

## Version 7.103

### December 2019

This document provides information regarding the Run-time Environment Installer GUI for Sentinel LDK and Sentinel HASP, including supported operating systems, enhancements, known compatibility issue, and issues resolved. ("Sentinel LDK" is the next generation of Sentinel HASP.)

The following topics are discussed:

>Operating Systems Supported

>Virtual Environments Supported

>Upgrading the Run-time Environment

>Installing the Run-time Environment

>Allowing Incoming Connections From Public Networks Using Port 1947

>Issues Related to Device Guard and Code Integrity Policies

>Enhancements and Issues Resolved in This Release

>Revision History

>Known Issues - Run-time Environment

## Operating Systems Supported

> Windows 7 SP1

> Windows 8.1 SP1

> Windows Server 2008 R2 SP1

> Windows Server 2012 R2

>Windows Server 2016

>Windows Server 2019

>Windows 10 IoT Enterprise 2019 LTSC

>Windows 10 Version 1903

NOTE Windows 10 Insider Preview builds are not supported.

The operating system versions listed in this section were tested by Gemalto and verified to be fully compatible with Sentinel LDK. For reasons of compatibility and security, Gemalto recommends that you always keep your operating system up to date with the latest fixes and service packs.

The installer detects the version of the operating system at run-time, before installing the relevant drivers.

## Virtual Environments Supported

For a list of the virtual environments supported, see "Supported Platforms for End Users" in the Sentinel LDK Release Notes.

The latest Release Notes can be seen at: http://sentinelldk.gemalto.com/LDKdocs/RN

Back to Topics

## Upgrading the Run-time Environment

When using the Installer GUI to upgrade the Run-time Environment, ensure that:

>No other Run-time Environment Installer is active.

>No other Run-time Environment components are active. Although the installation program terminates applications that are accessing the Run-time, it does not terminate running services. For example, if the Sentinel License Manager is running as a service, you must stop the service before upgrading the Run-time Environment.

Back to Topics

## Installing the Run-time Environment

>The Installer GUI detects the version of the operating system during Run-time Environment installation, before installing the relevant drivers.

>By default, Windows displays a User Account Control message during driver installation. The user must click Continue to continue the installation. Alternatively, the user can change the default setting from the Control Panel of their operating system.

>A log file of the installation process is written to aksdrvsetup.log in the Windows directory.

For additional information, see the topic “Upgrading Sentinel LDK Run-Time Environment (RTE) Installer” in the Sentinel EMS Configuration Guide.

Back to Topics

## Allowing Incoming Connections From Public Networks Using Port 1947

The Run-time Environment Installer adds a firewall rule named “Sentinel License Manager” that allowed incoming connections from private networks using port 1947.

You can manually allow access from public networks using this port, but Gemalto highly recommends against this.

If you do plan to allow incoming connections from public networks using port 1947, create a rule with a different name in order to prevent future RTE upgrades from removing this access.

Back to Topics

## Issues Related to Device Guard and Code Integrity Policies

The traditional method until now to protect against malicious application under Windows has been to trust the applications unless they were blocked by an antivirus or other security solution. Device Guard, available in Windows 10 Enterprise, implements a mode of operation in which the operating system trusts only applications that are authorized by your enterprise. You designate these trusted applications by creating code integrity policies.

You can maintain a whitelist of software that is allowed to run (a configurable code integrity policy), rather than trying to stay ahead of attackers by maintaining a constantly-updated list of "signatures" of software that should be blocked. This approach uses the trust-nothing model well known in mobile device operating systems.
Only code that is verified by Code Integrity, usually through the digital signature that you have identified as being from a trusted signer, is allowed to run. This allows full control over allowed code in both kernel and user mode.

Code integrity contains two primary components:

> kernel mode code integrity (KMCI)

> user mode code integrity (UMCI)

This section describes issues that arise and the workarounds when machines at the end user site are enabled with Device Guard, and the code integrity policy set to “enforce” mode.

NOTE The procedures described in this document should be performed by an IT professional who is familiar with Device Guard and code integrity policies.

### Issue 1: Windows blocks the installation of the Run-time Environment

During installation of the Run-time Environment on your computer, Windows displays a message similar to this: "Your organization used Device Guard to block this app. Contact your support person for more info."

Solution:

To install the Run-time Environment on a machine where Device Guard is enabled in enforce mode (which make use of PcaCertificate level code signing check), ensure that DigiCert is listed/added in the Signers list of the policy file.

Import the DigiCert Intermediate certificate to the trusted list of Intermediate Certification Authorities(ICA) store on the golden computer before creating code integrity policy.

A Digicert Intermediate certificate is available from https://aboutssl.org/digicert-trusted-root-authority-certificates/#intermediates. Under Intermediate Certificates, locate and download the DigiCert EV Code Signing CA (SHA2) certificate. You can also fetch this intermediate certificate from your trusted source.

To add the DigiCert Root Certificate

1.Download the certificate on the golden computer and double-click the certificate file. The Certificate dialog box is displayed.

2.Click Install Certificate. Follow the Certificate Install Wizard to complete the import of this certificate to the ICA store.

3.Run the steps to create a new or updated policy. This will allow Sentinel software to be installed without any issues on a machine where Device Guard is enabled.

Repeat the installation of the Run-time Environment.

### Issue 2: Protected application does not operate at the customer site

(LDK-17267) ) When you distribute applications that are protected with SL keys, the customized vendor library (haspvlib_vendorID.*) that are required for these applications are not signed. As a result, Device Guard does not allow the software to operate at the customer site.

Workaround A:

This workaround must be performed at the customer site.

Do the following to add an exception for the customized vendor library file in the code integrity policy:

1.Use Windows PowerShell in elevated mode to create a policy for the exception.

2.Use the Group Policy editor to deploy the policy file.

Each of these procedures is described below. For additional details, go to: https://technet.microsoft.com/en-us/itpro/windows/keep-secure/deploy-code-integrity-policies-steps?f=255&MSPPError=-2147217396

To create the policy for the exception

1. Open PowerShell in elevated mode.

2. Run the command to create a policy (referred to below as P1) in audit mode.

3. Deploy this policy.

4.Operate the protected application as you would normally.

5. Create another policy (referred to as P2) that captures audit information from the events log.

NOTE Before proceeding with the next step, review policy P2 carefully. This policy contains information about all the binaries that were used in your system while you operated the protected application. Any unwanted application that was executed during this time is logged in the policy. If not removed, any such application will be treated as a trusted binary.

6. Merge policies P1 and P2.

7. Disable audit mode.

8. Deploy the merged policy.

To deploy the policy file

1. Open the Group Policy editor by running GPEdit.msc.

2. Navigate to: Computer Configuration\Administrative Templates\System\Device Guard

3.Select Deploy Code Integrity Policy. Enable this setting by using the path to the relevant policy file created above.

Workaround B (not recommended):

This workaround must be performed at the customer site.

Before deploying the code integrity policy, disable UMCI (user mode code integrity) mode.

To accomplish this, run the following command in Windows PowerShell in elevated mode:

    Set-RuleOption -FilePath <Policy path> -Option 0 -Delete

### Issue 3: Vendor Tools fail to load

(SM-907) Sentinel LDK Vendor Tools fail to load. An error message is displayed, stating that a DLL, LIB, COM, or EXE file is not designed to run on Windows or that the DLL contains an error.

For example:

Workaround A:

Do the following to add a policy for the Sentinel LDK Vendor Tools in the code integrity policy file:

1.Use Windows PowerShell in elevated mode to create a policy for the Vendor Tools.

2.Use the Group Policy editor to deploy the policy file.

Each of these procedures is described below. For additional details, go to: https://technet.microsoft.com/en-us/itpro/windows/keep-secure/deploy-code-integrity-policies-steps?f=255&MSPPError=-2147217396

To create the policy for the Vendor Tools

1. Open PowerShell in elevated mode.

2. Run the command to create a policy (referred to below as P1) in audit mode.

3. Deploy this policy.

4. Execute all of the Vendor Tools that you will require at your site and perform all of the functions in these tools that you will require. If you miss any required Vendor Tools or Vendor Tool functions, the required entries will not be added in the new code integrity policy, and these tools or functions will generate an error message when they are eventually used.

5. Create another policy (referred to as P2) that captures audit information from the events log.

NOTE Before proceeding with the next step, review policy P2 carefully. This policy contains information about all the binaries that were used in your system while you operated the Vendor Tools. Any unwanted application that was executed during this time is logged in the policy. If not removed, any such application will be treated as a trusted binary.

6. Merge policies P1 and P2.

7. Disable audit mode.

8. Deploy the merged policy.

To deploy the policy file

1. Open the Group Policy editor by running GPEdit.msc.

2. Navigate to: Computer Configuration\Administrative Templates\System\Device Guard

3.Select Deploy Code Integrity Policy. Enable this setting by using the path to the relevant policy file created above.

Workaround B (not recommended):

Perform this workaround at your development site.

Before deploying the code integrity policy, disable UMCI (user mode code integrity) mode.

To accomplish this, run the following command in Windows PowerShell in elevated mode:

    Set-RuleOption -FilePath <Policy path> -Option 0 -Delete

No further actions are required.

### Issue 4: Digital signature removed from the RTE Installer

(SM-18780) When a user creates a Run-time Environment Installer using Sentinel EMS, the digital signature is removed from the Installer. As a result, Device Guard blocks the RTE Installer from executing.

If the vendor downloads the installer as an EXE file and signs it, Device Guard allows the installer to run, but the installation fails due to an unsigned DLL file called by haspdinst.exe.

Workaround:

Perform the procedure that follows.

1.Download the Run-time Environment Installer from the following URL in the Gemalto web site:

https://sentinelcustomer.gemalto.com/sentineldownloads/

2.Use the downloaded Installer to install the Run-time Environment.

3.Place a copy of the Vendor library (haspvlib_vendorID.*) in: %CommonProgramFiles(x86)%\Aladdin Shared\HASP\

(On a 32-bit machine, place the Vendor library in: %CommonProgramFiles%\Aladdin Shared\HASP\)

To work with Sentinel EMS, continue with the following additional steps:

4.In a Web browser, enter the following to start Admin Control Center: http://localhost:1947

5.On the Configuring Network Settings page, in the EMS URL field, enter the URL to access the Sentinel EMS Service.

6.Click Submit.

7.Proceed to work with Sentinel EMS as required.

As an alternative, you can use one of the workarounds provided above for issues 2 and 3.

Back to Topics

## Enhancements and Issues Resolved in This Release

### Enhancements in Version 7.103

Reference | Description
--- | ---
SM-51158 | Admin API now supports the use of HTTPS for communication with a remote Admin License Manager.
SM-12702 | A local or remote user can now use the "Sentinel Keys Available" page of Admin Control Center (instead of the RUS utility) to generate a fingerprint. Note: For Linux or Mac (where Admin Control Center is available), only SL AdminMode fingerprints can be generated.

### Issues Resolved in Version 7.103

Reference | Description
--- | ---
SM-66308 | Certain important security issues were resolved. For more information, see the reference to article KB0020564 in the Gemalto Security Updates page: https://sentinel.gemalto.com/technical-support/security-updates-sm/ Gemalto acknowledges and thanks Vladimir Dashchenko from Kaspersky Lab ICS CERT for responsible disclosure of these vulnerabilities.

Back to Topics

## Revision History

This section describes enhancements implemented and issues resolved in the last three major releases of Sentinel Run-time Environment.

The revision history for earlier versions of Sentinel Run-time Environment is available at: http://sentinelldk.gemalto.com/Default.htm

### Issues Resolved in Version 7.102

Reference | Description
--- | ---
SM-26322 | Certain important security issues were resolved. For more information, see the reference to article KB0020199 in the Gemalto Security Updates page: https://sentinel.gemalto.com/technical-support/security-updates-sm/ Gemalto acknowledges and thanks Artem Zinenko from Kaspersky Lab ICS CERT for responsible disclosure of these vulnerabilities.
SM-62256 | Under certain circumstances, it was possible to misuse detached licenses.
SM-64937 | When Sentinel EMS was used to create an RTE Installer after the Master Wizard was used multiple times to introduce Vendor keys, the vendor libraries included with the RTE Installer would have an incorrect date.
SM-65371 | The GUI-based RTE Installer would display an error screen when a .properties file existed in SysWOW64.

### Enhancements in Version 7.101

Reference | Description
--- | ---
SM-61960 | The Run-time Environment now supports controlling the generation of the License Manager ID files. This is done using the Enable Detaching of Licenses configuration check box in Admin Control Center. When selected, the License Manager generates ID files. When cleared, the License Manager stops generating any new ID files. However, the existing ID files are retained. By default, the Enable Detaching of Licenses check box is cleared.

### Issues Resolved in Version 7.101

Reference | Description
--- | ---
SM-62902 | Certain important security issues were resolved. For more information, see the reference to article KB0020074 in the Gemalto Security Updates page: https://sentinel.gemalto.com/technical-support/security-updates-sm/ Gemalto acknowledges and thanks the Blizzard Red Team for responsible disclosure of these vulnerabilities.

### Enhancements in Version 7.100

Reference | Description
--- | ---
SM-47546 | The Run-time Environment now supports the ability of the Licensing API to check remaining idle time before a protection key login session is terminated. Checking the remaining idle time does not reset the session.
SM-50812 | The Run-time Environment now supports improved protection against the misuse of computer restoration software (such as Deep Freeze).
SM-7269 SM-54601 | The Run-time Environment now supports protecting applications that run in a Docker container. The scheme VMType4 is supported for clone protection.

### Issues Resolved in Version 7.100

Reference | Description
--- | ---
SM-49346 | Under certain circumstances, the License Manager would generate a false-positive report of a virtual machine because some components of the Deep Freeze product were present on the machine.
SM-56397 | Given the following circumstances: >A license for a Product is detached from a customer's license server and applied on a different machine >In Sentinel EMS, the original entitlement for the Product is copied and used to create an update to the Product. The update is applied to the license server machine. >The detached license is canceled and returned to the license server. The number of available seats of the Product on the license server would not reflect that the license had been returned.
SM-57376 | In certain situations, an SL license would disappear after system reboot.
SM-56723 | When a machine was restored from sleep mode, a USB sharing violation error would occur if a HASP HL key was plugged into a USB HUB with an independent power supply.

### Issues Resolved in Version 7.92

Reference | Description
--- | ---
SM-50889 SM-50902 SM-50900 | Certain important security issues were resolved. For more information, see the reference to article KB0018794 in the Gemalto Security Updates page: https://sentinel.gemalto.com/technical-support/security-updates-sm/ Gemalto acknowledges and thanks Artem Zinenko from Kaspersky Lab ICS CERT for responsible disclosure of these vulnerabilities. As part of the resolution for these issues, Admin Control Center no longer supports importing external language packs (either online or offline). Translated user interface files are included in the RTE installer. The end user now selects the desired language for the interface by clicking the name of the language instead of clicking a country flag image.

### Issues Resolved in Version 7.91

Reference | Description
--- | ---
SM-43605 | Sentinel LDK drivers have been repackaged so that significant Windows 10 operating system upgrades will not impact existing SL AdminMode licenses.
SM-47103 | The Vlib search path for Runtime Environment versions 7.0 through 7.81 included the following paths: >For Windows x64: %CommonProgramFiles(x86)%\SafeNet Sentinel\Sentinel LDK\ %CommonProgramFiles(x86)%\Aladdin Shared\HASP\ >For Windows x86: %CommonProgramFiles%\SafeNet Sentinel\Sentinel LDK\ %CommonProgramFiles%\Aladdin Shared\HASP\ Support for the \SafeNet Sentinel\Sentinel LDK\ paths was discontinued in version 7.90. To reinstate support for vendors who have been placing their Vlib files in the \SafeNet Sentinel\Sentinel LDK\ directory, upon first use, Run-time Environment version 7.91 or later moves the Vlib files from the \SafeNet Sentinel\Sentinel LDK\ directory to the \Aladdin Shared\HASP\ directory.

### Enhancements in Version 7.90

Reference | Description
--- | ---
SM-17431 | The License Manager now supports the use of custom clone protection schemes.
SM-34308 | In Admin Control Center, the configuration parameter Allow Remote Access to ACC and Admin API has been split into two independent parameters: >Allow Remote Access to ACC >Allow Remote Access to Admin API This provide more granular control of access from a remote machine. You can now allow or deny access separately for Admin Control Center and for Admin API. (A corresponding split for configuration parameters was implemented in Sentinel Admin API.) When the License Manager is upgraded to version 7.90, each new parameter is assigned the value that was assigned to the original parameter. As a result, after the upgrade, there is no change in access granted.

### Enhancements in Version 7.81

Reference | Description
--- | ---
SM-18163 | The RTE Installer now provides more details in order to help ensure that installation of the RTE completes successfully. The Installer now differentiates between the following situations: >Installation of the RTE has succeeded. No restart is required. >Installation of the RTE cannot complete due to a lock on a required file. The RTE Installer attempts to rename the locked file in the background. If it succeeds, the installation will continue. If the rename attempt fails, the installer returns error 52. At this point, your code can call the new RTE Installer API function haspds_GetLockingProcessList to get the locking process name. You can then release the locked file and restart the RTE Installer.
SM-27901 | The revision history of all enhancements implemented and issues resolved for earlier versions of the RTE is now available online at: http://sentinelldk.safenet-inc.com/Default.htm
SM-30222 SM-30886 | Several security improvements have been implemented.

### Issues Resolved in Version 7.81

Reference | Description
--- | ---
SM-28148 | The hasp_login function would fail to log in to a HASP4 parallel port key (the function would not fail with HASP4 UBS keys). The login would fail with the error code HASP_HASP_NOT_FOUND = 7. This issue would occur with RTE version 7.52 and later.
SM-31010 | If the client connected using different IPv6 interfaces, the License Manager would sometimes count the sessions on a machine multiple times.

### Issues Resolved in Version 7.80

Reference | Description
--- | ---
SM-12155 | If a customer applies a V2C update from a remote machine that has the Vendor library but no license from the same vendor, the error returned was HASP_UPDATE_TOO_NEW, which was confusing. Now the error returned is HASP_KEYID_NOT_FOUND.
SM-18502 | Defining an excessive number of User Restrictions in Admin Control Center would cause the License Manager Service to fail.
SM-19981 | hasp_update would return an internal error for an HL Key when the license definition contains empty content in the default memory section.
SM-23609 | The RTE installer adds a firewall rule (named “Sentinel License Manager”) that, in the past, allowed incoming connections from any network, including public networks, using port 1947. Starting with RTE version 7.80, the firewall rule added by the RTE Installer does not allow incoming connections from public networks. If you are upgrading from an earlier version of RTE, the installer replaces the existing rule (that allows connections from public networks) with a rule that blocks such connections. You can manually allow access using this port from public networks, but Gemalto highly recommends against this. If you do plan to allow access from public networks using port 1947, create a rule with a different name in order to prevent future RTE upgrades from removing this access.
SM-25600 | The Run-Time Environment would require an excessive amount of time to install.
SM-26543 | Under certain circumstances, Sentinel License Manager would crash on the REST interface with long packets.
SM-9841 | HASP4 keys would stop working after the Run-time Environment was upgraded to v.7.54.

### Issues Resolved in Version 7.65

Reference | Description
--- | ---
SM-21408 | The Admin Control Center help system was missing information regarding the new “Idle Timeout of Session” configuration parameter.
SM-23320 | A possible security issue related to License Manager failure due to stack overflow on deep XML data (reported by Kaspersky) has been resolved.
SM-23402 | A possible security issue related to buffer overflow (reported by Kaspersky) has been resolved.
SM-23813 | A possible security issue that was reported by Kaspersky has been resolved.

### Enhancements in Version 7.63

Reference | Description
--- | ---
SM-13443 | When a Sentinel HL (HASP configuration) key or HASP HL key is attached to a Windows machine, the Run-time Environment is no longer installed automatically by Windows Update. It is now the software vendor’s responsibility to ensure that the Run-time Environment is installed when required.
SM-13505 | In the past, the timeout for an idle License Manager session was fixed at 12 hours. You can now set the timeout to any value between 10 minutes and 720 minutes (12 hours). The timeout value can be set as follows: >In Admin Control Center, on the Basic Configuration page. Use the Idle Timeout of Session parameter. >In the hasplm.ini file. Assign the timeout value to idle_session_timeout_mins.
SM-14894 | Admin Control Center now adds the update counter in C2V files in clear text - for example: <update_counter>5</update_counter> It is no longer necessary to decode the C2V file in order to view this information.
SM-19483 | Admin Control Center now recognizes the new V2CP format to update protection keys. This supports planned enhancements in Sentinel LDK v.7.8.

### Issues Resolved in Version 7.63

Reference | Description
--- | ---
SM-15922 | Admin Control Center no longer requires the <?xml header in a V2C file.
SM-17175 | After system reboot/service restart, an SL AdminMode detached license would disappear from a recipient machine that had no other licenses.
SM-18015 | On some machines, the License Manager service would start before the Secure Storage driver is loaded. This would cause the Secure Storage to become corrupted. Now, the License Manager service waits for the Secure Storage driver to start.
SM-18302 | Cancelling a detached SL AdminMode license from the recipient VM machine would fail with the HASP_VM_DETECTED error.
SM-18502 | In Admin Control Center, defining too many users in the User Restrictions field would cause the License Manager to fail.

### Enhancements in Version 7.61

Reference | Description
--- | ---
SM-5318 | The Run-time Environment now supports the use of the VMType3 clone protection scheme.

### Enhancements in Version 7.60

Reference | Description
--- | ---
SM-1286 | You can now enter the URL to access Sentinel EMS in your Web browser without changing the EMS URL to lowercase.
SM-901 | Admin Control Center (under Windows) can now display and apply updates to local SL UserMode keys. (Session information and certificate information for SL UserMode keys is not displayed.)
SM-4237 | To display SL UserMode keys in Admin Control Station, License Manager runs an additional process (hasplmv) on the machine. If you are willing to accept that SL UserMode keys will not be displayed, you have the option to prevent hasplmv from executing by clearing the relevant check box on the Configuration page in Admin Control Center.
SM-6525 | In the past, Admin Control Center and Admin API provided a configuration parameter that determined whether a remote user could access and perform actions in Admin Control Center. However, this parameter did not control remote access to Admin API. Now, the parameter Allow Remote Access to ACC and Admin API (in Admin Control Center) and the tag <accremote> (in Admin API) control remote access to both Admin Control Center and Admin API.

### Issues Resolved in Version 7.60

Reference | Description
--- | ---
LDK-12145 | When a data file is protected with Version 2 data protection mode for Android platforms: If, for any reason (for example, no license was found), the protected application was not able to decrypt the protected data file, no error message was generated to explain why the file cannot be opened.
SM-513 | Under Windows 10, a physical machine would be detected as a virtual machine when only Hyper-V Hypervisor is enabled.
SM-515 | It was possible to rehost a cloned license to another machine.
SM-518 | The Diagnostics report in Admin Control Center (Diagnostics > Generate Report) displays information on "Recent Clients" and "Recent Users". Each entry contained a time stamp but not a date stamp. The report has been corrected to display both a time stamp and a date stamp for each entry.
SM-6102 | When building a Run-Time Environment installer using Wix, an error message similar to the following was generated: Invalid product version '7.53.1.66350' in package HASP_Setup.msi'. When included in a bundle, all product version fields in an MSI package must be less than 65536. This error no longer occurs.
SM-942 | Under certain circumstances, Sentinel LDK License Manager Service would crash. The exception code would map to STATUS_STACK_OVERFLOW in __chkstk API.

Back to Topics

## Known Issues

Reference | Description
--- | ---
SM-68016 | After you upgrade the Run-time Environment, Admin Control Center might show a dummy key id for Key type - "HASP Placeholder" Workaround: Refresh Admin Control Center.
SM-36385 | After Windows 7 is upgraded to Windows 8, the user is not able to use existing SL licenses or to install new SL licenses. Workaround: After you upgrade from Windows 7 to Windows 8, reinstall the Run-time Environment.
SM-20626 | When installing the RTE on a machine where Fabula Tech USB over Network is installed, installation of the RTE hangs. Workaround: Disconnect the HL key before running the RTE installer.
SM-907 | Sentinel LDK Vendor Tools fail to load under Windows 10 when Device Guard is enabled and the Code Integrity policy is set to "enforce". An error message is displayed regarding a certain DLL, stating that the DLL is not designed to run on Windows or that the DLL contains an error. For more information, see Issues Related to Device Guard and Code Integrity Policies.
LDK-17302 LDK-13953 LDK-14971 | Given the following circumstances at a customer site: 1. One machine has Run-time Environment version 7.51. 2. A second machine has a version of Run-time Environment that is earlier than 7.51. 3. The customer performs rehost of a license repeatedly between the two machines. 4. An update is applied to the license on either of these machines. A rehost operation sometimes fails with the message HASP_REHOST_ALREADY_APPLIED. Workaround: Obtain a new SL license from the software vendor for the protected application on the target machine. Before attempting any additional rehost procedure, install the latest Run-time Environment on both machines.
LDK-17267 | The License Manager fails to load vlibs under Windows 10 when Device Guard is enabled and the Code Integrity policy is set to “enforce”. For more information, see Issues Related to Device Guard and Code Integrity Policies.
LDK-8480 | With some new USB chipsets, it is possible that the API hasp_update() call, used to update the firmware of Sentinel HL keys to version 3.25, will generate the HASP_BROKEN_SESSION return code, even if the firmware is correctly updated. (This issue does not occur with Sentinel HL Driverless keys with firmware version 4.x.) Workaround: Install the latest Run-time Environment. The automatic firmware update feature of the License Manager will automatically update the firmware of the key the first time that the key is connected, without the need to call hasp_update().
LDK-2471 | Sentinel Licensing API: On a computer with the Nvidia chip set GeForce 7025/nForce 630a, and where the CPU is AMD Athlon 64 X2, the hasp_read and hasp_encrypt functions may fail with error 39, HASP_BROKEN_SESSION. This problem only exists with HASP HL keys with Firmware version 3.25. Workaround 1: On the computer described above, when error 39 is returned, call the hasp_read or hasp_encrypt function again. It is not necessary to call hasp_login again. Workaround 2: Use Sentinel HL keys with Firmware version 4.2x.
12506 | Sentinel LDK communicates via TCP and UDP on port 1947. This port is IANA-registered exclusively for this purpose. At the end user site, the firewall must be configured so that communication via this port is not blocked.

Back to Topics

© Gemalto 2019. All rights reserved. Gemalto, the Gemalto logo, are trademarks and service marks of Gemalto and are registered in certain countries.

DocID 118 Revision 1912-4